gcg2 2% gif
 Use which GIF version:

  GIF87a

  GIF89a

 Please choose one ( * GIF89a * )

 Enter GIF89a output filename (* /dev/tty15 *) $program$.gif
 Enter image width (* 640 *) 800
 Enter image height (* 428 *) 600
 Plotting Configuration set to:

       Language: gifd

         Device: GIF89a

  Port or Queue: $program$.gif

     Image Size: 800 x 600

